When using the new receiver script you will have to change the variables passed into a recieveSignal() call in simulations:

rxer.receiveSignal(txer,thetas,phis,channel.awgn,**X**,noise\_power=10)

^^ add X

X = 1 means awgn

X = 2 means rlhf

X = 3 means both

**Channel options:**

channel.awgn() uses Gausian white noise

channel.rlhf() uses Raleigh fading

channel.both() uses both Gausian white noise and Raleigh fading